Brandon Pollack

Lab Summary

Prelab Questions:

1. The iron should touch the PC board where the lead will go and the lead itself. The unmelted solder should touch the joint.
2. 5-7 bare wire turns. 1-1.5 turns of insulated wire, cut 1 inch of wire.
3. 2 surface mount chips, 12 jumpers, 3 SIPS
4. Makeup policy is that a missed lab is your drop, and you can drop any lab, but only one. If there is an emergency case with proof for BOTH cases in the case of two missed labs, then it can be made up.
5. [eel4744uf@gmail.com](mailto:eel4744uf@gmail.com), 30 minutes late, 10 to still take quiz.
6. 65%

Problems:

Nope

List of Files:

Summary.doc

Amelstudio

Future applications:

Now I can do prelabs properly and know lab policies.