Brandon Pollack

Lab6

Summary

Problems encountered:

Busy flag would not work for me in my LCD, so I had to resort to using a delay.

Future Application:

It is my understanding that most 2 line LCD abide by the same standard, so I am well prepared to sue them for many things now.

Files:

QAR

Lab6\_BRP

Lab6\_part2\_BRP

Lab6\_part3\_BRP

EBI\_INITS

Schematics